##### [API function]

## FSOUND_GetCurrentLevels

Returns a left and right VU/Level reading at the current position of the specified channel.
Levels are are only supported for software channels.

DLL_API signed char F_API FSOUND_GetCurrentLevels(
int channel,
F_FLOAT_API *l,
F_FLOAT_API *r
);

### Parameters

channel | Channel number/handle to retrieve left and right level from.
l | Pointer to a floating point value to store left level, between 0 and 1.
r | Pointer to a floating point value to store right level, between 0 and 1.

### Return Value

On success, TRUE is returned.
On failure, FALSE is returned.

### Remarks

By default this function is only point sampled and not latency adjusted (it will appear to trigger ahead of when you hear the sound).
To fix this and get a 'perfect' set of levels in realtime, use FSOUND_INIT_ACCURATEVULEVELS with FSOUND_Init.
-------------------
To get an overall VU reading for all sounds, add all VU values for each channel together, and then clip at 1.0.
Another (harder) way is to write a dsp unit that reads from the mixbuffer being passed into it.
Note: A true 'VU' should be smoothed, but in case people were after more accuracy than a smoothed value, it was decided to return the raw amplitude, and let the user smooth the result in their own way.
___________________
Supported on the following platforms : Win32, WinCE, Linux, Macintosh, XBox, PlayStation 2, GameCube

### See Also

FSOUND_GetAmplitude , FSOUND_Init

This document copyright ©Firelight Technologies, Pty, Ltd, 1999-2002. All rights reserved.
Generated Thu Dec 15 17:31:29 2005 by SourceDoc v0.10, the automated source code documenter.