##### [API function]

## FSOUND_SPU2_GetRawAddress

Gets the raw SPU2 offset inside the SPU2 memory space from the handle returned from FSOUND_SPU2_Alloc

unsigned int F_API FSOUND_SPU2_GetRawAddress(
void *iopptr
);

### Parameters

iopptr | Pointer to the IOP based sound ram handle.

### Return Value

The SPU2 address of the data allocated. This is not directly addressable.
The only way to get data to this address is to DMA it from the EE to the IOP first, then from the IOP to SRAM.

### Remarks

___________________
Supported on the following platforms : PlayStation 2

### See Also

FSOUND_SPU2_Alloc , FSOUND_SPU2_Free

This document copyright ©Firelight Technologies, Pty, Ltd, 1999-2002. All rights reserved.
Generated Thu Dec 15 17:31:35 2005 by SourceDoc v0.10, the automated source code documenter.